Bradley Davis

This document explains the function of the EPS, its schematic level design, its board level design, and its functional testing

EPS

Electrical Power Subsystem Design

Revision: 3.0.3



Table of Contents

[1 Introduction 4](#_Toc25149769)

[1.1 Function 4](#_Toc25149770)

[1.2 Requirements 4](#_Toc25149771)

[2 Detailed Description 5](#_Toc25149772)

[2.1 Functional Block Diagram 5](#_Toc25149773)

[2.1.1 Power Input 5](#_Toc25149774)

[2.1.2 Energy Storage 5](#_Toc25149775)

[2.1.3 Power Output 6](#_Toc25149776)

[2.1.4 PMIC 6](#_Toc25149777)

[2.1.5 Monitoring 6](#_Toc25149778)

[2.2 Schematic 6](#_Toc25149779)

[2.2.1 Isolated Grounds 6](#_Toc25149780)

[2.2.2 Power Rails 7](#_Toc25149781)

[2.2.3 Input Switching 7](#_Toc25149782)

[2.2.4 Battery & Battery Protection 7](#_Toc25149783)

[2.2.5 Separation Switching 8](#_Toc25149784)

[2.2.6 3.3V Regulation 8](#_Toc25149785)

[2.2.7 Output Switching 9](#_Toc25149786)

[2.2.8 Current Monitoring 9](#_Toc25149787)

[2.2.9 Voltage Monitoring 9](#_Toc25149788)

[2.2.10 Temperature Monitoring 10](#_Toc25149789)

[2.2.11 PMIC 10](#_Toc25149790)

[2.2.12 I²C Bus 10](#_Toc25149791)

[2.2.13 SPI Bus 11](#_Toc25149792)

[2.2.14 Analog Voltage Reference and Supply 11](#_Toc25149793)

[2.2.15 Mechanical Features 11](#_Toc25149794)

[2.3 Board 11](#_Toc25149795)

[2.3.1 Layer Stack-Up 12](#_Toc25149796)

[2.3.2 Layout Constraints 12](#_Toc25149797)

[3 Testing 14](#_Toc25149798)

[3.1 Before First Power-On Check 14](#_Toc25149799)

[3.1.1 Test Instructions 14](#_Toc25149800)

[3.1.2 Test Data 14](#_Toc25149801)

[3.2 Separation Switching 15](#_Toc25149802)

[3.2.1 Test Instructions 15](#_Toc25149803)

[3.2.2 Test Data 16](#_Toc25149804)

[3.2.3 Test Notes 16](#_Toc25149805)

[3.3 Power Rails 16](#_Toc25149806)

[3.3.1 Test Instructions 16](#_Toc25149807)

[3.3.2 Test Data 16](#_Toc25149808)

[3.4 Input Switching 17](#_Toc25149809)

[3.4.1 Test Instructions 18](#_Toc25149810)

[3.4.2 Test Data 18](#_Toc25149811)

[3.4.3 Test Notes 19](#_Toc25149812)

[3.5 Output Switching 19](#_Toc25149813)

[3.5.1 Test Instructions 19](#_Toc25149814)

[3.5.2 Test Data 19](#_Toc25149815)

[3.5.3 Test Notes 21](#_Toc25149816)

[3.6 Battery Charging 21](#_Toc25149817)

[3.6.1 Test Instructions 21](#_Toc25149818)

[3.6.2 Test Data 21](#_Toc25149819)

[3.7 Battery Protection 21](#_Toc25149820)

[3.7.1 Discharge Overcurrent 21](#_Toc25149821)

[3.7.2 Load Short Circuit 23](#_Toc25149822)

[3.7.3 Charge Overcurrent 24](#_Toc25149823)

[3.7.4 Charge Overvoltage 26](#_Toc25149824)

[3.7.5 Discharge Undervoltage 27](#_Toc25149825)

[3.8 3.3V Regulator 29](#_Toc25149826)

[3.8.1 Voltage 29](#_Toc25149827)

[3.8.2 Ripple and Noise 30](#_Toc25149828)

[3.8.3 Efficiency 31](#_Toc25149829)

[3.8.4 Current Limit 32](#_Toc25149830)

[3.9 Load Response - Battery 33](#_Toc25149831)

[3.9.1 Test Instructions 33](#_Toc25149832)

[3.9.2 Test Data 33](#_Toc25149833)

[3.9.3 Test Notes 36](#_Toc25149834)

[3.10 Load Response – 3.3V Regulator 36](#_Toc25149835)

[3.10.1 Test Instructions 36](#_Toc25149836)

[3.10.2 Test Data 36](#_Toc25149837)

[3.10.3 Test Notes 41](#_Toc25149838)

[3.11 I²C Bus 41](#_Toc25149839)

[3.11.1 Test Instructions 41](#_Toc25149840)

[3.11.2 Test Data 42](#_Toc25149841)

[3.11.3 Test Notes 42](#_Toc25149842)

[3.12 Current Monitoring 42](#_Toc25149843)

[3.12.1 Test Instructions 42](#_Toc25149844)

[3.12.2 Test Data 42](#_Toc25149845)

[3.12.3 Test Notes 43](#_Toc25149846)

[3.13 Voltage Monitoring 43](#_Toc25149847)

[3.13.1 Test Instructions 44](#_Toc25149848)

[3.13.2 Test Data 44](#_Toc25149849)

[3.14 Temperature Monitoring 44](#_Toc25149850)

[3.14.1 Test Instructions 44](#_Toc25149851)

[3.14.2 Test Data 44](#_Toc25149852)

[3.15 Analog Voltage Reference 44](#_Toc25149853)

[3.15.1 Voltage 45](#_Toc25149854)

[3.15.2 Ripple and Noise 45](#_Toc25149855)

[3.16 PMIC Programming 46](#_Toc25149856)

[3.16.1 Test Instructions 46](#_Toc25149857)

[3.16.2 Test Data 46](#_Toc25149858)

[3.16.3 Test Notes 46](#_Toc25149859)

# Introduction

This document explains how the EPS will fulfil the following Functions and conform to the following Requirements. This document refers to the EPS version 3.0 and Solar Panel version 2.0.

## Function

The Electrical Power Subsystem (EPS) is responsible for the following:

* Accumulating energy
* Regulating voltage
* Distributing power

## Requirements

The system requirements and EPS design requirements can be found [on GitHub](https://github.com/CougsInSpace/CougSat1-Readme/blob/master/CougSat1-Requirements.pdf).

# Detailed Description

This section references the EPS [schematic](https://github.com/CougsInSpace/CougSat1-Hardware/blob/master/CougSat1-PowerBoard/Documentation/EPS.pdf). Page numbers will be listed and may have coordinates listed (number and letter combination found around the frame).

## Functional Block Diagram

The block diagram can be found on the first page of the schematic.

### Power Input

Energy is captured from the Sun using an array of photovoltaic cells[[1]](#footnote-1). These cells are mounted onto solar panels that adjust the voltage and current to acceptable levels for direct charging of lithium-ion batteries[[2]](#footnote-2). These criteria are up to and up to [[3]](#footnote-3) per battery. Furthermore, power can be inputted from the umbilical[[4]](#footnote-4) using the same criteria as the solar panels. The umbilical will only be used whilst on the ground. The PMIC will automatically monitor the charging and disable current paths to follow the prescribed charging, see Energy Storage for more details. Most lithium-ion charging curves indicate voltage up to and current up to ; however, the EPS will limit to and to preserve battery health[[5]](#footnote-5). Replacing the batteries on the EPS whilst in orbit is very difficult.

The solar panel and umbilical inputs are routed through a balance switching matrix before entering the batteries. This allows the PMIC to switch every cell going to either or both batteries[[6]](#footnote-6).

### Energy Storage

The EPS stores energy from the solar panels in batteries to fulfil high instantaneous power demands and any power demands during periods of eclipse[[7]](#footnote-7). Each battery has a protection IC that protects against the following faults:

* Overcharge
* Over-discharge
* Charge overcurrent
* Discharge overcurrent
* Load short-circuit detection

The PMIC will monitor and regulate the temperature of the batteries. The batteries (and power inputs) disconnect from the rest of the EPS via separation switches and the RBF switch[[8]](#footnote-8).

### Power Output

The EPS has two separate rails for distribution: unregulated from the batteries and [[9]](#footnote-9). There are two regulators[[10]](#footnote-10), one per battery. Most loads are connected via the [backplane](https://github.com/CougsInSpace/CougSat1-Hardware/blob/master/CougSat1-Backplane/Documentation/Backplane-Design.pdf) and are individually switched between either source (power chain A or B) or turned off, and current monitored[[11]](#footnote-11). The PMIC controls these turning on and off, the switch for chain A or B is automatically performed.

There is a single load that cannot be disconnected from the regulators: the PMIC[[12]](#footnote-12). This ensures there is at least one processor that can turn on the rest of the satellite. The outputs’ default states are off such that the PMIC must turn the loads on, this prevents glitching as the PMIC boots up. The power rail going to the In-Flight JTAG Reprogrammer ([IFJR](https://github.com/CougsInSpace/CougSat1-Hardware/blob/master/CougSat1-AvionicBoard/Documentation/IFJR-Design.pdf)) is logical ORed with *JTAG\_EN\_PMIC* such that if the IFJR is programming the PMIC, its GPIO goes high impedance but the IFJR remains powered on to avoid corruption.

### PMIC

The Power Management IC (PMIC) is the microprocessor monitoring and operating the EPS[[13]](#footnote-13). Only one PMIC exist as adding redundant processors adds complexity that could reduce reliability. It communicates over I²C to Command and Data Handling subsystem ([C&DH](https://github.com/CougsInSpace/CougSat1-Hardware/blob/master/CougSat1-AvionicBoard/Documentation/C&DH-Design.pdf))[[14]](#footnote-14) via the backplane and to its monitoring sensors directly. It collects sensor information and transfers this to the C&DH to be included in a telemetry packet to Ground[[15]](#footnote-15). The C&DH may also send commands. For example, enter safe mode by switching off specific subsystems[[16]](#footnote-16).

### Monitoring

The PMIC, through ADCs, monitors current, and voltage at various locations and temperature of various components, indicated on the block diagram[[17]](#footnote-17).

## Schematic

### Isolated Grounds

On page 2 of the schematic (D1), are the four isolated grounds found on the EPS. Power ground *(PGND)* is directly connected to the backplane and most of the power chain. The other grounds are shorted to *PGND* using a resistor rated up to , the expected current is less than each. Digital ground *(DGND)* connects to the digital circuity including the PMIC and Monitoring circuits. Analog ground *(AGND)* connects to analog monitoring circuits including the ADCs, their voltage reference, and the thermistors. Chassis ground *(CHASSIS)* is connected to the Mechanical Features including bolt holes and the card rails.

### Power Rails

Page 2 of the schematic illustrates all the power rails on the EPS. Notice how most components of the power chain can be routed to the other chain to increase redundancy. The expected current consumptions are derived from the [energy budget](https://github.com/CougsInSpace/CougSat1-Hardware/blob/master/CougSat1-PowerBoard/Documentation/EnergyBudget.pdf). The limit of less than per rail is imposed by the backplane with current limiters[[18]](#footnote-18).

#### Always-On Rail

There is one rail that is always-on and cannot be switched off, except with the Separation Switching. This provide power for the PMIC as the PMIC cannot be allowed to turn off or other subsystems may not be able to be turned on. It is *3.3V* (page 5, B5). They use “ideal diodes”[[19]](#footnote-19) to OR the power together from both power chains, whichever rail has a higher voltage provides the current.

### Input Switching

A matrix of ideal diodes[[20]](#footnote-20) (page 3) switch the solar panel inputs and umbilical input to either battery. The lower voltage battery receives the current first until both batteries have the same voltage. Their enable pin are connected to the PMIC for enabling or disabling charging. To reduce the number of enable pins, cells on the opposite side of the satellite share an enable. The increased control over individual cells is not important as the opposite side cell will be in shadow and okay if disabled.

As the GPIO of the PMIC defaults to high impedance input during boot up (every reset will enter this state). The IC includes an active pullup on its enable pin so an external one is not needed for when the PMIC is off.

The power inputs are placed in parallel with the batteries such that the loads will draw from the power inputs before drawing from the batteries.

### Battery & Battery Protection

The batteries[[21]](#footnote-21) (page 4, B2 & B5) are 18650 lithium-ion. The chemistry was chosen for its high volumetric and mass energy densities. A specific cell has not been chosen; a long-term study is required. The EPS will be compatible with most cells.

The batteries are protected by dedicated lithium-ion single-cell protection ICs[[22]](#footnote-22) (page 4, B2 & B5). They measure the current passing through the battery by measuring the voltage between pins 4 & 6. With the Rds(on) of the MOSFET[[23]](#footnote-23) and the shunt resistor, the IC prevents against of overcurrent. The IC also prevents against of over-voltage and of under-voltage.

The batteries are thermally connected to a heater and Temperature Monitoring thermistor. The heater is a TO-220 resistor which generates up to of heat. A lower resistance resistor may be exchanged for more heating capabilities, a thermal test will indicate this need. The heater can be driven at lower duty cycle, through PWM, to reduce the average output power.

### Separation Switching

The separation switches (connected via the backplane) or the RBF pin switch (page 4, D3) disconnect the batteries and power input from the rest of the power chain. Either of the switches apply a pull down to the gate of a MOSFET that inverts the signal to another MOSFET that interrupts the power chain. When the umbilical is connected, and voltage is applied, it drives the MOSFETs the opposite way to connect the power chain. In the default state (no switches depressed or umbilical connected) a weak pull up to the batteries (through ORing diodes) keeps the MOSFETS driven to connect the power chain.

Connected to the separation switches and RBF pin switch is a capacitor and limiting resistor such that the time constant is buffered with a unity gain buffer[[24]](#footnote-24). The PMIC measures the voltage across the capacitor. When the PMIC boots up, it will check this voltage is decide if it is powering up after a reset (the capacitor will still be charged) or after a deployment (the capacitor will be discharged).

### 3.3V Regulation

The 3.3V regulators (page 5) are switching mode, buck topology. The controller[[25]](#footnote-25) automatically senses the output voltage and adjusts the switching parameters to keep the output at . The controller was chosen for its small package and ability to output duty cycle such that when the input drops below , the output will follow the voltage of the input.

The large package Multi-Layer Ceramic Capacitors (MLCC, input and output filtering) are placed in series such that one was to fail short, they would not compromise the power chain. The small package and tantalum capacitors are not likely to fail due to mechanical vibration.

On the drain of the switching MOSFETs (page 5, A3 & C3) are snubber circuits that absorb and suppress transients thus reducing the output noise.

The switching MOSFETs and inductors (page 5, A3 & C3) are thermally connected to a thermistor for Temperature Monitoring and an optional heatsink if a thermal test indicates they need additional heat dissipation.

### Output Switching

The output switching (pages 6, 7) uses ideal diodes[[26]](#footnote-26) that automatically switch between power chain A or B, whichever is higher voltage, and have an integrated current limit. The PMIC controls each one individual between off and on with automatic switching. All rail’s default state is off for when the PMIC is off and not driving the enable signals. Th IFJR’s power rail is also (logical OR) enabled when the *JTAG\_EN\_PMIC* is on as described in Power Input.

Most outputs go into the backplane for distribution to their connected subsystem. The *PR\_DEPLOY* output (for releasing deployable mechanisms) and *PV\_3.3V* (for the solar panel monitoring circuits) connect to their load via wire harness (page 3).

### Current Monitoring

At various locations, the power chain has shunt resistors with current shunt amplifiers[[27]](#footnote-27) connected to ADCs to monitor the current. Those locations are:

* Batteries: charging/discharging (page 4, B2 & B5)
* Power chain input (page 4, A2 & A5)
* 3.3V regulator input (page 5, A3 & C3)
* 3.3V regulator output (page 5, A5 & C5)

Output switching ideal diodes[[28]](#footnote-28) have a current limit set by resistor whose current is proportional to the diode’s current. This voltage is measured by an ADC to sense the current.

The solar panels monitor their own current and the PMIC communicates to them via the wire harness (page 3).

### Voltage Monitoring

At various locations, the power chain is probed for the voltage using one of the ADCs. Those locations are:

* Batteries (page 4, A3 & A4)
* 3.3V regulator output (page 5, A6 & C6)
* Umbilical input (page 3, C2)

The solar panels monitor their own voltages and the PMIC communicates to them via the wire harness (page 3).

### Temperature Monitoring

At various locations, the temperature is monitored using thermistors and one of the ADCs. Those locations are:

* Batteries (page 4, B3 & B4)
* 3.3V regulator switching components (page 5, A4 & C4)
* Input switching (page 3, D3)
* Output switching (page 6, D4; page 7, D4)
* PMIC (page 9, C4)
* Various locations of the PCB (page 11, A5:A6)
* Each ADC has an integrated temperature sensor

### PMIC

The PMIC (page 9) is a microcontroller from the STM32 low power family[[29]](#footnote-29). It was chosen for its ease of programming, and low power consumption. Since the PMIC is essentially just controlling GPIO and talking over two I²C Buses and a SPI Bus, the features of higher end processors are not needed.

#### Programming Connections

During testing, the PMIC is programmed via Serial Wire Debug[[30]](#footnote-30) (SWD, page 9, D5). The process of programming is made simple with just a single pin header and a robust software utility. In orbit, the PMIC can be programmed via JTAG[[31]](#footnote-31). The [In-Flight JTAG Reprogrammer](https://github.com/CougsInSpace/CougSat1-Hardware/blob/master/CougSat1-AvionicBoard/Documentation/IFJR-Design.pdf) (IFJR) connects via the backplane, through a tri-state buffer/logic level converter[[32]](#footnote-32) (page 8, A1:B2). The IFJR can enable or disable the tri-state buffer which essentially disconnects the JTAG interface from the PMIC (it outputs high impedance), allowing the SWD to program. The logic level conversion feature is not used.

### I²C Bus

The PMIC has two I²C buses (page 9). One is for the EPS monitoring and control devices. The other is to communicate with the C&DH. On the EPS bus, the PMIC is the master served by the attached devices. Busses that communicate with devices on different power rails go through a tri-state buffer[[33]](#footnote-33), such that when the device is powered off, its ESD diodes do not hold the bus low preventing communication with the other devices on the bus.

#### ADCs

There are nine ADCs[[34]](#footnote-34) connected to the PMIC, each with eight single-ended inputs. Four are on the EPS (page 11). There is one on each solar panel. The ADC was chosen for its low power, small package, SAR architecture and up to nine addresses. The list of address follow:

* [0x58] EPS-0 (page 11, A2)
* [0x5C] EPS-1 (page 11, B2)
* [0x5E] EPS-2 (page 11, C2)
* [0x56] EPS-3 (page 11, B5)
* [0x40] EPS-4 (page 11, C5)
* [0x54] PV0 (+Z) (page 3, A1)
* [0x50] PV1 (-Y) (page 3, A3)
* [0x44] PV2 (-X) (page 3, B1)
* [0x46] PV3 (+Y) (page 3, B3)

#### Backplane to C&DH

The PMIC is a slave to the C&DH. See the [interface document](https://github.com/CougsInSpace/CougSat1-Software/blob/master/CougSat1-PMIC/docs/PMICInterface.pdf) for details.

### SPI Bus

The PMIC has one SPI bus (page 9) to communicate with three ADCs[[35]](#footnote-35). These ADCs have a high bit count for resolution when measuring critical nodes including power chain currents and power chain voltages. Each ADC has its own select pin.

### Analog Voltage Reference and Supply

Each ADC has its own analog reference of with high temperature stability, not requiring a high precision external reference. For the thermistors, they are sourced from this analog reference with a unity gain buffer[[36]](#footnote-36) to allow higher current draw (page 11, B4 & D4).

The EPS has an analog voltage supply (page 11, D2) which is fed by the always-on *3.3V* rail filtered with a ferrite bead and capacitors. Precision is not required as all ADCs use the precision voltage reference for calibration. This is the source for the analog unity gain buffers and ADCs.

### Mechanical Features

The RBF pin holder (page 4, D1) and 3.3V Regulation heatsink (page 5, B1 & D1) mount directly to the EPS board using bolts. These holes are conductive and connected directly to *CHASSIS*, see Isolated Grounds. The EPS also slots into the structure using rails[[37]](#footnote-37) which are also conductive and connected directly to chassis ground. Each of the holes have a capacitor and resistor connecting to power ground which will absorb transients.

## Board

The board shall conform to the dimensions specified by the [CougSat Module Standard](https://github.com/CougsInSpace/CougSat1-Hardware/blob/master/CougSat1-Backplane/Documentation/CougSatModuleStandard.pdf).

### Layer Stack-Up

The board shall be four layered with ENIG finish, see Figure 1. Only through vias shall be used. The external copper weight shall be and the internal copper weight shall be .

| Layer | Thickness | Primary Function |
| --- | --- | --- |
| 1 (top) |  | SMD components, signal traces |
| Prepreg |  |  |
| 2 |  | Ground planes |
| Core |  |  |
| 3 |  | Power planes |
| Prepreg |  |  |
| 4 (bottom) |  | Signal traces |

Figure 1: Stack-Up

### Layout Constraints

Unless specified in the following subsections, all signals shall use the default parameters below. Signals in the following subsections do not include their sense signals unless otherwise specified. Trace width can be broken if a trace needs to bottleneck down to a pin, the bottleneck shall be minimized.

Trace width:

Vias: , unlimited count

Separation:

Length: unlimited

Devices with specific placement and routing considerations are called out on the schematic, see “CAD Note:”

#### Solar Panel Inputs – PV\_IN[0:3][A:B], PGND

PGND applies to between the solar panel headers and the backplane

Trace width: ( on internal layers)

#### Umbilical Input – UMB\_IN, PGND

PGND applies to between the umbilical header and the backplane

Trace width: ( on internal layers)

#### Battery Input – VIN-[A:B], PGND

PGND applies to between the solar panel headers and the backplane

Trace width: ( on internal layers)

#### Battery Connections – BP\_VSS-[A:B], BP\_VSS-I[A:B], VBATT-[A:B], PGND

PGND applies to between the low side battery protection MOSFETs and the backplane.

Trace width: ( on internal layers)

Vias: five per layer change

#### SMPS Switching Node – 3.3V\_ISENS-[A:B], 3.3V\_REG\_BUCK\_NODE-[A:B]

Trace width:

Vias: No vias

Minimize RF emission

#### SMPS Output – 3.3V\_I-[A:B], 3.3V-[A:B]

The traces can taper down once loads branch off and less than three loads remain.

Trace width: ( on internal layers)

Vias: three per layer change

#### SMPS Ground – PGND

PGND applies to between the filtering capacitors and the backplane.

Trace width: ( on internal layers)

#### Rail Output Channels – PR\_3.3V-[0:12], PR\_BATT-[0:6], PR\_BH-[0:1]

Trace width: ( on internal layers)

#### Deployables Output – PR\_DEPLOY

Trace width: ( on internal layers)

#### JTAG – JTAG-[TCK, TDI, TDO, TMS], BUS\_JTAG-[TCK, TDI, TDO, TMS]

Length: Each node shall be length matched

Stubs:

#### I2C – I2C\_[SDA, SCL], BUS\_I2C\_[SDA, SCL, IRQ]

Length: Each node shall be length matched

Stubs:

# Testing

All tests shall be performed at room temperature and not under vacuum unless otherwise specified. If any modifications are performed, take note. Include enough information to understand circuit behavior and for others to replicate the results. Include any software written to execute the test and link it in the test notes section. Save all software, waveforms, etc. in a subfolder of the board’s test folder for each test[[38]](#footnote-38).

* Waveforms shall be captured whenever appropriate
* Have the event take fill the screen (for fast events, zoom in; for slow events, zoom out)
* Label each channel accurately
* Only have bandwidth limiting if necessary for the test (this applies to the oscilloscope and probe settings)
* If ringing or overshoot occurs, use a ground spring or differential probe

Results location: <https://github.com/CougsInSpace/CougSat1-Hardware/tree/master/CougSat1-PowerBoard/Testing/EPS.3.0>

Common test instructions can be found on the [wiki](http://cougs.space/wiki).

Note: In the following sections, applying a source means to connect a power supply limited to and . The actual voltage and current may be less than this.

## Before First Power-On Check

**Configuration: Mr. Fitzgerald**

This test is required to be executed before batteries are attached and before any external power is applied to the EPS.

### Test Instructions

Measure the resistance of various points in reference to *PGND* located at the backplane. Measure the resistance across each current shunt resistor before installing. This is informational only; the resistance of the current shunt resistor is used to calibrate the Current Monitoring.

Measure low value resistors via a constant current source and voltmeter in a four-wire setup to minimize noise. Measure current limit set resistor via a constant current source through the limiter and a voltmeter on the resistor, this compensates the limiter’s gain.

### Test Data

| Node | Resistance |  | Node | Resistance |
| --- | --- | --- | --- | --- |
| *VIN-A* |  |  | *VIN-B* |  |
| *VBATT-A* |  |  | *VBATT-B* |  |
| *VIN* |  |  | *3.3V* |  |
| *3.3V-A* |  |  | *3.3V-B* |  |
| *I2C\_SCL* |  |  | *I2C\_SDA* |  |
| *BUS\_I2C\_SCL* |  |  | *BUS\_I2C\_SDA* |  |
| *PV\_I2C\_SCL* |  |  | *PV\_I2C\_SDA* |  |
| *BP\_VSS-A* |  |  | *BP\_VSS-B* |  |
| *AVDD* |  |  |  |  |

| Net | Resistor | Value |  | Net | Resistor | Value |
| --- | --- | --- | --- | --- | --- | --- |
| *PR\_3.3V-0* | R81 |  |  | *PR\_3.3V-1* | R79 |  |
| *PR\_3.3V-2* | R76 |  |  | *PR\_3.3V-3* | R73 |  |
| *PR\_3.3V-4* | R71 |  |  | *PR\_3.3V-5* | R70 |  |
| *PR\_3.3V-6* | R67 |  |  | *PR\_3.3V-7* | R65 |  |
| *PR\_3.3V-8* | R63 |  |  | *PR\_3.3V-9* | R60 |  |
| *PR\_3.3V-10* | R59 |  |  | *PR\_3.3V-11* | R58 |  |
| *PR\_3.3V-12* | R57 |  |  | *PR\_BATT-0* | R56 |  |
| *PR\_BATT-1* | R55 |  |  | *PR\_BATT-2* | R54 |  |
| *PR\_BATT-3* | R51 |  |  | *PR\_BATT-4* | R50 |  |
| *PR\_BATT-5* | R45 |  |  | *PR\_BATT-6* | R39 |  |
| *PR\_BH-0* | R38 |  |  | *PR\_BH-1* | R26 |  |
| *PR\_DEPLOY-0* | R74 |  |  | *PR\_DEPLOY-1* | R10 |  |
| *3.3V* | R24 |  |  | *3.3V\_PV* | R12 |  |

## Separation Switching

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Separation Switching.

### Test Instructions

Discharge or charge the batteries to before executing this test. Insert the RBF pin, wait at least , remove the RBF pin. Measure *PWR\_CTRL\_SW, VBATT-A, VBATT-B,* and *EJECT\_TIMER\_BUF.*

### Test Data

| Insert the RBF pin, wait at least , remove the RBF pin. | | | |
| --- | --- | --- | --- |
| Operation | Capture *PWR\_CTRL\_SW, VBATT-A, VBATT-B,* and *EJECT\_TIMER* | Passing Criteria | Pass / Fail |
| Insertion |  | *VBATT-A* and *VBATT-B* fall < within ,  *EJECT\_TIMER* falls < within | Pass |
| Removal |  | *VBATT-A* and *VBATT-B* rise > within , *EJECT\_TIMER* rises > between and | Pass |

### Test Notes

Channel 1 is *EJECT\_TIMER*, channel 3 is *VBATT-A.*

## Power Rails

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Power Rails.

### Test Instructions

Discharge or charge the batteries to before executing this test. With the PMIC not running code, upload a blank image or assert its reset pin, and the RBF pin inserted, apply power to each input one at a time as follows:

* to the solar panel inputs
* to the umbilical input

Ensure that both batteries are receiving the power.

### Test Data

| Apply to PV\_IN-0A | | | |
| --- | --- | --- | --- |
| Battery | Power | Passing Criteria | Pass / Fail |
| A |  | Power > | Pass |
| B |  | Power > | Pass |

| Apply to PV\_IN-0B | | | |
| --- | --- | --- | --- |
| Battery | Power | Passing Criteria | Pass / Fail |
| A |  | Power > | Pass |
| B |  | Power > | Pass |

| Apply to PV\_IN-1A | | | |
| --- | --- | --- | --- |
| Battery | Power | Passing Criteria | Pass / Fail |
| A |  | Power > | Pass |
| B |  | Power > | Pass |

| Apply to PV\_IN-1B | | | |
| --- | --- | --- | --- |
| Battery | Power | Passing Criteria | Pass / Fail |
| A |  | Power > | Pass |
| B |  | Power > | Pass |

| Apply to PV\_IN-2A | | | |
| --- | --- | --- | --- |
| Battery | Power | Passing Criteria | Pass / Fail |
| A |  | Power > | Pass |
| B |  | Power > | Pass |

| Apply to PV\_IN-2B | | | |
| --- | --- | --- | --- |
| Battery | Power | Passing Criteria | Pass / Fail |
| A |  | Power > | Pass |
| B |  | Power > | Pass |

| Apply to PV\_IN-3A | | | |
| --- | --- | --- | --- |
| Battery | Power | Passing Criteria | Pass / Fail |
| A |  | Power > | Pass |
| B |  | Power > | Pass |

| Apply to PV\_IN-3B | | | |
| --- | --- | --- | --- |
| Battery | Power | Passing Criteria | Pass / Fail |
| A |  | Power > | Pass |
| B |  | Power > | Pass |

| Apply to UMB\_IN | | | |
| --- | --- | --- | --- |
| Battery | Power | Passing Criteria | Pass / Fail |
| A |  | Power > | Pass |
| B |  | Power > | Pass |

## Input Switching

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Input Switching.

### Test Instructions

Discharge or charge the batteries to before executing this test. Drive each input switch to the following states while applying a source:

* *Both Off*
* *A On*
* *B On*
* *Both On*

Ensure each channel is properly routing the power.

### Test Data

| Configure each input channel to *Both Off*.  Apply a source to the input under test | | | | |
| --- | --- | --- | --- | --- |
| Channel | Battery A Power | Battery B Power | Passing Criteria | Pass / Fail |
| *PV\_IN-0A* |  |  |  | Pass |
| *PV\_IN-0B* |  |  |  | Pass |
| *PV\_IN-1A* |  |  |  | Pass |
| *PV\_IN-1B* |  |  |  | Pass |
| *PV\_IN-2A* |  |  |  | Pass |
| *PV\_IN-2B* |  |  |  | Pass |
| *PV\_IN-3A* |  |  |  | Pass |
| *PV\_IN-3B* |  |  |  | Pass |

| Configure each input channel to *A On*.  Apply a source to the input under test | | | | |
| --- | --- | --- | --- | --- |
| Channel | Battery A Power | Battery B Power | Passing Criteria | Pass / Fail |
| *PV\_IN-0A* |  |  |  | Pass |
| *PV\_IN-0B* |  |  |  | Pass |
| *PV\_IN-1A* |  |  |  | Pass |
| *PV\_IN-1B* |  |  |  | Pass |
| *PV\_IN-2A* |  |  |  | Pass |
| *PV\_IN-2B* |  |  |  | Pass |
| *PV\_IN-3A* |  |  |  | Pass |
| *PV\_IN-3B* |  |  |  | Pass |

| Configure each input channel to *B On*.  Apply a source to the input under test | | | | |
| --- | --- | --- | --- | --- |
| Channel | Battery A Power | Battery B Power | Passing Criteria | Pass / Fail |
| *PV\_IN-0A* |  |  |  | Pass |
| *PV\_IN-0B* |  |  |  | Pass |
| *PV\_IN-1A* |  |  |  | Pass |
| *PV\_IN-1B* |  |  |  | Pass |
| *PV\_IN-2A* |  |  |  | Pass |
| *PV\_IN-2B* |  |  |  | Pass |
| *PV\_IN-3A* |  |  |  | Pass |
| *PV\_IN-3B* |  |  |  | Pass |

| Configure each input channel to *Both On*.  Apply a source to the input under test | | | | |
| --- | --- | --- | --- | --- |
| Channel | Battery A Power | Battery B Power | Passing Criteria | Pass / Fail |
| *PV\_IN-0A* |  |  |  | Pass |
| *PV\_IN-0B* |  |  |  | Pass |
| *PV\_IN-1A* |  |  |  | Pass |
| *PV\_IN-1B* |  |  |  | Pass |
| *PV\_IN-2A* |  |  |  | Pass |
| *PV\_IN-2B* |  |  |  | Pass |
| *PV\_IN-3A* |  |  |  | Pass |
| *PV\_IN-3B* |  |  |  | Pass |

### Test Notes

Negative power indicated discharging, the EPS circuits (PMIC and such) were on and consuming power.

## Output Switching

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Output Switching.

### Test Instructions

Discharge or charge the batteries to before executing this test. Drive each output switch to the following states while applying a resistive load:

* *Off*
* *On*

Note: *PR\_BH-[0,1]* already have a resistive load and do not need an external load applied.

### Test Data

| Configure each output channel to *Both Off*.  Apply a resistive load to the output under test | | | | |
| --- | --- | --- | --- | --- |
| Channel | Battery A Power | Battery B Power | Passing Criteria | Pass / Fail |
| *PR\_3.3V-PV* |  |  |  | Pass |
| *PR\_3.3V-0* |  |  |  | Pass |
| *PR\_3.3V-1* |  |  |  | Pass |
| *PR\_3.3V-2* |  |  |  | Pass |
| *PR\_3.3V-3* |  |  |  | Pass |
| *PR\_3.3V-4* |  |  |  | Pass |
| *PR\_3.3V-5* |  |  |  | Pass |
| *PR\_3.3V-6* |  |  |  | Pass |
| *PR\_3.3V-7* |  |  |  | Pass |
| *PR\_3.3V-8* |  |  |  | Pass |
| *PR\_3.3V-9* |  |  |  | Pass |
| *PR\_3.3V-10* |  |  |  | Pass |
| *PR\_3.3V-11* |  |  |  | Pass |
| *PR\_3.3V-12* |  |  |  | Pass |
| *PR\_BATT-0* |  |  |  | Pass |
| *PR\_BATT-1* |  |  |  | Pass |
| *PR\_BATT-2* |  |  |  | Pass |
| *PR\_BATT-3* |  |  |  | Pass |
| *PR\_BATT-4* |  |  |  | Pass |
| *PR\_BATT-5* |  |  |  | Pass |
| *PR\_BATT-6* |  |  |  | Pass |
| *PR\_DEPOLY-0* |  |  |  | Pass |
| *PR\_DEPOLY-1* |  |  |  | Pass |
| *PR\_BH-0* |  |  |  | Pass |
| *PR\_BH-1* |  |  |  | Pass |

| Configure each output channel to *On*.  Apply a resistive load to the output under test | | | | |
| --- | --- | --- | --- | --- |
| Channel | Battery A Power | Battery B Power | Passing Criteria | Pass / Fail |
| *PR\_3.3V-PV* |  |  |  | Pass |
| *PR\_3.3V-0* |  |  |  | Pass |
| *PR\_3.3V-1* |  |  |  | Pass |
| *PR\_3.3V-2* |  |  |  | Pass |
| *PR\_3.3V-3* |  |  |  | Pass |
| *PR\_3.3V-4* |  |  |  | Pass |
| *PR\_3.3V-5* |  |  |  | Pass |
| *PR\_3.3V-6* |  |  |  | Pass |
| *PR\_3.3V-7* |  |  |  | Pass |
| *PR\_3.3V-8* |  |  |  | Pass |
| *PR\_3.3V-9* |  |  |  | Pass |
| *PR\_3.3V-10* |  |  |  | Pass |
| *PR\_3.3V-11* |  |  |  | Pass |
| *PR\_3.3V-12* |  |  |  | Pass |
| *PR\_BATT-0* |  |  |  | Pass |
| *PR\_BATT-1* |  |  |  | Pass |
| *PR\_BATT-2* |  |  |  | Pass |
| *PR\_BATT-3* |  |  |  | Pass |
| *PR\_BATT-4* |  |  |  | Pass |
| *PR\_BATT-5* |  |  |  | Pass |
| *PR\_BATT-6* |  |  |  | Pass |
| *PR\_DEPOLY-0* |  |  |  | Pass |
| *PR\_DEPOLY-1* |  |  |  | Pass |
| *PR\_BH-0* |  |  |  | Pass |
| *PR\_BH-1* |  |  |  | Pass |

### Test Notes

Positive power indicated discharging, the EPS circuits (PMIC and such) were on and consuming power which is the quiessceint load.

## Battery Charging

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Battery & Battery Protection.

### Test Instructions

Discharge or charge the batteries to before executing this test. With the PMIC not running code, upload a blank image or assert its reset pin, and the RBF pin inserted, apply a source to the umbilical input. Measure the change in voltage after and validate the battery is charging.

Note: Measure the voltage without the external source applied

### Test Data

| Apply a source to the umbilical input  Measure the change in voltage after | | | | | |
| --- | --- | --- | --- | --- | --- |
| Battery | Initial Voltage | Final Voltage |  | Passing Criteria | Pass / Fail |
| A |  |  |  |  | Pass |
| B |  |  |  |  | Pass |

## Battery Protection

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Battery & Battery Protection.

### Discharge Overcurrent

#### Test Instructions

Discharge or charge the batteries to before executing this test. For each battery, apply an increasing load to *VBATT* until *DOUT* transitions low. Remove the load and attach the charger. Measure *COUT*, and *DOUT*. Ensure the output switches are configured to the correct battery.

Note: Connect all the power outputs together to share the overcurrent.

#### Test Data

| Apply an increasing load to *PR\_BATT* outputs until *DOUT* transitions low | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture *COUT*, *DOUT* | Trigger Current | Passing Criteria | Pass / Fail |
| A |  |  |  | Pass |
| B |  |  |  | Pass |

| Remove the load and attach the battery charger | | | |
| --- | --- | --- | --- |
| Battery | Capture *COUT*, *DOUT* | Passing Criteria | Pass / Fail |
| A |  | Operation Restored | Pass |
| B |  | Operation Restored | Pass |

#### Test Notes

Yellow is COUT, purple is DOUT. Since COUT is referenced to PGND and the IC disconnected PGND and battery ground, COUT appears to fall but its ground is rising (note it does not fall a large voltage). This also explains the oscillations.

### Load Short Circuit

#### Test Instructions

Discharge or charge the batteries to before executing this test. For each battery, apply a short between *VBATT* and *PGND*. Remove this short. Measure *COUT*, and *DOUT*. Ensure the output switches are configured to the correct battery.

#### Test Data

| Apply a short between *VBATT* and *PGND* | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture *COUT*, *DOUT* | Trigger Delay | Passing Criteria | Pass / Fail |
| A |  |  |  | Pass |
| B |  |  |  | Pass |

| Remove the load and attach the battery charger | | | |
| --- | --- | --- | --- |
| Battery | Capture *COUT*, *DOUT* | Passing Criteria | Pass / Fail |
| A |  | Operation Restored | Pass |
| B |  | Operation Restored | Pass |

#### Test Notes

Yellow is COUT, purple is DOUT. Since COUT is referenced to PGND and the IC disconnected PGND and battery ground, COUT appears to fall but its ground is rising (note it does not fall a large voltage). This also explains the oscillations.

### Charge Overcurrent

#### Test Instructions

Discharge or charge the batteries to before executing this test. For each battery, apply a source to the power inputs with increasing current until *COUT* transitions low. Decrease the current until *COUT* transitions high. Measure the *COUT*, and *DOUT*. Ensure the output switches are configured to the correct battery.

Note: Connect all the power inputs together to share the overcurrent.

#### Test Data

| Apply a source to the power inputs with an increasing current until *COUT* transitions low | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture *COUT*, *DOUT* | Trigger Current | Passing Criteria | Pass / Fail |
| A |  |  |  | Pass |
| B |  |  |  | Pass |

| Remove the battery charger | | | |
| --- | --- | --- | --- |
| Battery | Capture *COUT*, *DOUT* | Passing Criteria | Pass / Fail |
| A |  | Operation Restored | Pass |
| B |  | Operation Restored | Pass |

#### Test Notes

Yellow is COUT, purple is DOUT

### Charge Overvoltage

#### Test Instructions

Discharge or charge the batteries to before executing this test. For each battery, apply a source to the umbilical with increasing voltage until *COUT* transitions low. Remove the source and apply a resistive load until *COUT* transitions high. Measure the battery voltage, *COUT*, and *DOUT*. Ensure the output switches are configured to the correct battery.

Note: The overvoltage protection delay is typically 1.25s

#### Test Data

| Apply a source to the umbilical input with an increasing voltage until *COUT* transitions low | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture *COUT*, *DOUT* | Trigger Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  | Pass |
| B |  |  |  | Pass |

| During overvoltage protection, apply a resistive load until *COUT* transitions high | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture *COUT*, *DOUT* | Trigger Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  | Pass |
| B |  |  |  | Pass |

#### Test Notes

Yellow is COUT, purple is DOUT

### Discharge Undervoltage

#### Test Instructions

Discharge or charge the batteries to before executing this test. For each battery, apply a resistive load to *VBATT* until *DOUT* transitions low. Remove the load and apply a source to the umbilical input until *DOUT* transitions high. Measure the battery voltage, *COUT*, and *DOUT*. Ensure the output switches are configured to the correct battery.

Note: The undervoltage protection delay is typically 144ms

#### Test Data

| Apply a resistive load to *VBATT* until D*OUT* transitions low | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture *COUT*, *DOUT* | Trigger Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  | Pass |
| B |  |  |  | Pass |

| During undervoltage protection, apply a source to the umbilical input until *DOUT* transitions high | | | | |
| --- | --- | --- | --- | --- |
| Battery | Capture *COUT*, *DOUT* | Trigger Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  | Pass |
| B |  |  |  | Pass |

#### Test Notes

Yellow is COUT, purple is DOUT

## 3.3V Regulator

**Results: Fail**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in 3.3V Regulation. More information on measuring noise/ripple as well as using an oscilloscope can be found on the Power Team page of the Wiki under Tutorials and Resources

### Voltage

#### Test Instructions

Discharge or charge the batteries to before executing this test. With the RBF pin removed, measure the voltage of each 3.3V regulator under no load and under a resistive load. Ensure the output switches are configured to the correct regulator.

Note: Measure the DC component with PLC[[39]](#footnote-39) > 100

#### Test Data

| Measure the voltage of each 3.3V regulator under no load and under a resistive load | | | | |
| --- | --- | --- | --- | --- |
| Regulator | No Load Voltage | Load Voltage | Passing Criteria | Pass / Fail |
| A |  |  |  | Pass |
| B |  |  |  | Pass |

### Ripple and Noise

#### Test Instructions

Discharge or charge the batteries to before executing this test. With the RBF pin removed, measure the ripple of each 3.3V regulator whilst under a resistive load.

Note: Measure the RMS value of the AC component with

#### Test Data

| Measure the RMS voltage ripple and noise of each 3.3V regulator whilst under a resistive load. | | | |
| --- | --- | --- | --- |
| Regulator | Capture the ripple | Passing Criteria | Pass / Fail |
| A | DMM: |  |  |
| B | DMM: |  |  |

#### Test Notes

The controller on B gets damaged after of high usage (transients?). The layout needs to be updated and regulator A needs to be tested for latent failures of the same type.

### Efficiency

#### Test Instructions

Measure the efficiency of 3.3V regulator A whilst under a resistive loads and with input voltage.

Note: , measure the power across the input and output current shunt resistors.

#### Test Data

| Measure the efficiency of 3.3V regulator A whilst under a resistive load and input voltage. | | | | | |
| --- | --- | --- | --- | --- | --- |
| Input Voltage | Power In | Power Out | Efficiency | Passing Criteria | Pass / Fail |
| 3.0V |  |  |  |  |  |
| 3.3V |  |  |  |  |  |
| 3.7V |  |  |  |  |  |
| 4.1V |  |  |  |  |  |

| Measure the efficiency of 3.3V regulator A whilst under a resistive load and input voltage. | | | | | |
| --- | --- | --- | --- | --- | --- |
| Input Voltage | Power In | Power Out | Efficiency | Passing Criteria | Pass / Fail |
| 3.0V |  |  |  |  |  |
| 3.3V |  |  |  |  |  |
| 3.7V |  |  |  |  |  |
| 4.1V |  |  |  |  |  |

| Measure the efficiency of 3.3V regulator A whilst under a resistive load and input voltage. | | | | | |
| --- | --- | --- | --- | --- | --- |
| Input Voltage | Power In | Power Out | Efficiency | Passing Criteria | Pass / Fail |
| 3.0V |  |  |  |  |  |
| 3.3V |  |  |  |  |  |
| 3.7V |  |  |  |  |  |
| 4.1V |  |  |  |  |  |

| Measure the efficiency of 3.3V regulator A whilst under a resistive load and input voltage. | | | | | |
| --- | --- | --- | --- | --- | --- |
| Input Voltage | Power In | Power Out | Efficiency | Passing Criteria | Pass / Fail |
| 3.0V |  |  |  |  |  |
| 3.3V |  |  |  |  |  |
| 3.7V |  |  |  |  |  |
| 4.1V |  |  |  |  |  |

| Measure the efficiency of 3.3V regulator A whilst under a resistive load and input voltage. | | | | | |
| --- | --- | --- | --- | --- | --- |
| Input Voltage | Power In | Power Out | Efficiency | Passing Criteria | Pass / Fail |
| 3.0V |  |  |  |  |  |
| 3.3V |  |  |  |  |  |
| 3.7V |  |  |  |  |  |
| 4.1V |  |  |  |  |  |

| Measure the efficiency of 3.3V regulator A whilst under a resistive load and input voltage. | | | | | |
| --- | --- | --- | --- | --- | --- |
| Input Voltage | Power In | Power Out | Efficiency | Passing Criteria | Pass / Fail |
| 3.0V |  |  |  |  |  |
| 3.3V |  |  |  |  |  |
| 3.7V |  |  |  |  |  |
| 4.1V |  |  |  |  |  |

| Measure the efficiency of 3.3V regulator A whilst under a resistive load and input voltage. | | | | | |
| --- | --- | --- | --- | --- | --- |
| Input Voltage | Power In | Power Out | Efficiency | Passing Criteria | Pass / Fail |
| 3.0V |  |  |  |  |  |
| 3.3V |  |  |  |  |  |
| 3.7V |  |  |  |  |  |
| 4.1V |  |  |  |  |  |

#### Efficiency Plot

Create a plot of current versus efficiency with each input voltage.

#### Test Notes

The electronic load to do efficiency testing easily is not available. The efficiency of EPS 2.1 (same circuit) passed. The efficiency will be tested on EPS 3.1.

### Current Limit

#### Test Instructions

Discharge or charge the batteries to before executing this test. For each regulator, apply an increasing load to *3.3V* until the current no longer increases. Measure voltage and current of the rail. Ensure the output switches are configured to the correct battery.

Note: Connect all the power outputs together to share the overcurrent. The load will likely be increased by adding more resistors in parallel or decrease the load resistance. Be sure to not exceed per channel.

#### Test Data

| Apply an increasing load to *3.3V* outputs until the current no longer increases | | | |
| --- | --- | --- | --- |
| *3.3V* | Max Current | Passing Criteria | Pass / Fail |
| A |  |  |  |
| B |  |  |  |

#### Test Notes

The electronic load to do load testing easily is not available. The current limit of EPS 2.1 (same circuit) passed. The current limit will be tested on EPS 3.1. Furthermore regulator B is breaking on EPS 3.0 which affects the current limit.

## Load Response - Battery

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Output Switching and Battery & Battery Protection.

### Test Instructions

Discharge or charge the batteries to before executing this test. Apply the following loads to both *VBATT* rails.

* No load to resistive load
* resistive load to no load
* No load to MLCC[[40]](#footnote-40)
* resistive load adding MLCC

Capture the battery current and the voltage on *PR\_BATT-6* with a MLCC to simulate a subsystem. Validate the EPS does not misoperate in any way. Ensure the output switches are configured to the correct battery.

### Test Data

| To each *VBATT* rail, apply no load to resistive load | | | |
| --- | --- | --- | --- |
| *VBATT* | Capture current of the battery and the voltage of *PR\_BATT-6* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *VBATT* rail, apply resistive load to no load | | | |
| --- | --- | --- | --- |
| *VBATT* | Capture current of the battery and the voltage of *PR\_BATT-6* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *VBATT* rail, apply no load to MLCC | | | |
| --- | --- | --- | --- |
| *VBATT* | Capture current of the battery and the voltage of *PR\_BATT-6* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *VBATT* rail, apply resistive load and add MLCC | | | |
| --- | --- | --- | --- |
| *VBATT* | Capture current of the battery and the voltage of *PR\_BATT-6* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

### Test Notes

Yellow is *PR\_BATT-6*, purple is *VBATT-A* current, blue is *VBATT-B* current. .

## Load Response – 3.3V Regulator

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Output Switching and 3.3V Regulation.

### Test Instructions

Discharge or charge the batteries to before executing this test. Apply the following loads to both *3.3V* rails:

* No load to resistive load
* resistive load to no load
* No load to MLCC
* resistive load adding MLCC
* No load to short circuit
* Short circuit to no load
* resistive load to short circuit
* Short circuit to resistive load
* Short circuit continuous

Capture the battery current and the voltage on *PR\_3.3V-11* with a MLCC to simulate a subsystem. Validate the EPS does not misoperate in any way. Ensure the output switches are configured to the correct battery.

### Test Data

| To each *3.3V* rail and *PR\_3V3\_0*, apply no load to resistive load | | | |
| --- | --- | --- | --- |
| *3.3V* | Capture current of the regulator and the voltage of *PR\_3.3V-11* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *3.3V* rail, apply resistive load to no load | | | |
| --- | --- | --- | --- |
| *3.3V* | Capture current of the regulator and the voltage of *PR\_3.3V-11* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *3.3V* rail, apply no load to MLCC | | | |
| --- | --- | --- | --- |
| *3.3V* | Capture current of the regulator and the voltage of *PR\_3.3V-11* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *3.3V* rail, apply resistive load and add MLCC | | | |
| --- | --- | --- | --- |
| *3.3V* | Capture current of the regulator and the voltage of *PR\_3.3V-11* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *3.3V* rail, apply no load to short circuit | | | |
| --- | --- | --- | --- |
| *3.3V* | Capture current of the regulator and the voltage of *PR\_3.3V-11* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *3.3V* rail, apply short circuit to no load | | | |
| --- | --- | --- | --- |
| *3.3V* | Capture current of the regulator and the voltage of *PR\_3.3V-11* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *3.3V* rail, apply short circuit continuous load | | | |
| --- | --- | --- | --- |
| *3.3V* | Capture current of the regulator and the voltage of *PR\_3.3V-11* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *3.3V* rail, apply resistive load to short circuit | | | |
| --- | --- | --- | --- |
| *3.3V* | Capture current of the regulator and the voltage of *PR\_3.3V-11* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

| To each *3.3V* rail, apply short circuit to resistive load | | | |
| --- | --- | --- | --- |
| *3.3V* | Capture current of the regulator and the voltage of *PR\_3.3V-11* | Passing Criteria | Pass / Fail |
| A |  | No misoperation | Pass |
| B |  | No misoperation | Pass |

### Test Notes

Yellow is *PR\_3.3-11*, purple is *3.3V-A* current, blue is *3.3V-B* current. .

## I²C Bus

**Results: Fail**

**Configuration:**

This test evaluates the circuit described in I²C Bus.

### Test Instructions

Discharge or charge the batteries to before executing this test. At the test points of each I2C bus, validate signal integrity. The PMIC should generate random I2C traffic on each bus. A slave device might need to be added to execute this test.

### Test Data

| At the test points of the *I2C* bus, validate the following timing parameters | | | |
| --- | --- | --- | --- |
| Bus | Capture the *SDA* and *SCL* lines | Passing Criteria | Pass / Fail |
| *I2C* |  | Signal Integrity | Pass |
| *PV\_I2C* |  | Signal Integrity |  |
| *BUS\_I2C0* |  | Signal Integrity |  |
| *BUS\_I2C* |  | Signal Integrity |  |

### Test Notes

Other devices on the other busses is not available currently. It will be tested once they become available

## Current Monitoring

**Results: Fail**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Current Monitoring.

### Test Instructions

Discharge or charge the batteries to before executing this test. Apply a resistive load to *PR\_DEPLOY-0* and *3.3V-A*. Compare the current measured by the EPS and a DMM.

Note:


### Test Data

| Apply a resistive load to *PR\_DEPLOY-0*. Compare the current measured by the EPS and a DMM | | | | | |
| --- | --- | --- | --- | --- | --- |
| Load | EPS Current | DMM Current | Error | Passing Criteria | Pass / Fail |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

| Apply a resistive load to *VIN\_OUT-B*. Compare the current measured by the EPS and a DMM | | | | | |
| --- | --- | --- | --- | --- | --- |
| Load | EPS Current | DMM Current | Error | Passing Criteria | Pass / Fail |
|  |  |  |  |  | Pass |
|  |  |  |  |  | Pass |
|  |  |  |  |  | Pass |
|  |  |  |  |  | Pass |
|  |  |  |  |  | Pass |
|  |  |  |  |  | Pass |
|  |  |  |  |  | Pass |

### Test Notes

The current mirrors in 60-0014 output high impedance and the ADC’s input impedance affects its ability to limit current. Every sample brings the node down to zero. This negates the current limiting feature. See the plot below (purple trace) which shows a jump in voltage due to a decrease in impedance.



## Voltage Monitoring

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Voltage Monitoring.

### Test Instructions

Discharge or charge the batteries to before executing this test. Compare the voltage measured by the EPS and a DMM on the following signals:

* *UMB\_IN*
* *VBATT-A*
* *3.3V-A*

Note:

### Test Data

| Compare the voltage measured by the EPS and a DMM | | | | | |
| --- | --- | --- | --- | --- | --- |
| Signal | EPS Voltage | DMM Voltage | Error | Passing Criteria | Pass / Fail |
| *UMB\_IN* |  |  |  |  | Pass |
| *VBATT-A* |  |  |  |  | Pass |
| *3.3V-A* |  |  |  |  | Pass |

## Temperature Monitoring

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Temperature Monitoring.

### Test Instructions

Discharge or charge the batteries to before executing this test. Compare the temperature measured by the EPS and a thermometer on the following temperature sensors:

* Battery A
* PMIC
* +X+Y

Note:

### Test Data

| Compare the temperature measured by the EPS and a thermometer | | | | | |
| --- | --- | --- | --- | --- | --- |
| Sensor | EPS Temperature | Thermometer Temperature | Error | Passing Criteria | Pass / Fail |
| Battery A |  |  |  |  | Pass |
| PMIC |  |  |  |  | Pass |
| Regulator A |  |  |  |  | Pass |

## Analog Voltage Reference

**Results: Pass**

**Configuration: Mr. Fitzgerald**

This test evaluates the circuit described in Analog Voltage Reference and Supply.

### Voltage

#### Test Instructions

Discharge or charge the batteries to before executing this test. With the RBF pin removed, measure the voltage of *VREF*.

Note: Measure the DC component with PLC[[41]](#footnote-41) > 100

#### Test Data

| Measure the voltage of each voltage reference | | | | |
| --- | --- | --- | --- | --- |
| Signal | Test Point | Voltage | Passing Criteria | Pass / Fail |
| *ADC\_REF-0* | *TP41* |  |  | Pass |
| *ADC\_REF-1* | *TP14* |  |  | Pass |
| *ADC\_REF-2* | *TP30* |  |  | Pass |
| *ADC\_REF-3* | *TP5* |  |  | Pass |
| *ADC\_REF-4* | *TP9* |  |  | Pass |
| *ADC\_REF-5* | *TP24* |  |  | Pass |
| *ADC\_REF-6* | *TP10* |  |  | Pass |
| *ADC\_REF-7* | *TP39* |  |  | Pass |
| *AVREF-0* | *TP13* |  |  | Pass |
| *AVREF-1* | *TP38* |  |  | Pass |

### Ripple and Noise

#### Test Instructions

Discharge or charge the batteries to before executing this test. With the RBF pin removed, measure the ripple of *VREF*.

Note: Measure the RMS value of the AC component with

#### Test Data

| Measure the RMS voltage ripple and noise of each voltage reference | | | | |
| --- | --- | --- | --- | --- |
| Signal | Test Point | Voltage | Passing Criteria | Pass / Fail |
| *ADC\_REF-0* | *TP41* |  |  | Pass |
| *ADC\_REF-1* | *TP14* |  |  | Pass |
| *ADC\_REF-2* | *TP30* |  |  | Pass |
| *ADC\_REF-3* | *TP5* |  |  | Pass |
| *ADC\_REF-4* | *TP9* |  |  | Pass |
| *ADC\_REF-5* | *TP24* |  |  | Pass |
| *ADC\_REF-6* | *TP10* |  |  | Pass |
| *ADC\_REF-7* | *TP39* |  |  | Pass |
| *AVREF-0* | *TP13* |  |  | Pass |
| *AVREF-1* | *TP38* |  |  | Pass |

#### Test Notes

6 ½ Digit DMM displayed which is .

## PMIC Programming

**Results: Fail**

**Configuration:**

This test evaluates the circuit described in Programming Connections.

### Test Instructions

Discharge or charge the batteries to before executing this test. Connect a SWD programmer to the SWD header and upload an image, validate the PMIC is properly programmed. Connect a JTAG programmer to the backplane and upload an image, validate the PMIC is properly programmed.

Note: Follow the programming instructions on the [wiki](http://cougs.space/wiki).

### Test Data

| Program the PMIC via SWD and JTAG, validate the PMIC is properly programmed | | |
| --- | --- | --- |
| Programmer | Passing Criteria | Pass / Fail |
| SWD | PMIC properly programmed | Pass |
| JTAG | PMIC properly programmed |  |

### Test Notes

JTAG programmer is not available right now. JTAG programming will be tested once we have one.

1. Requirement EPS-010 [↑](#footnote-ref-1)
2. For details on charging lithium-ion batteries, <http://batteryuniversity.com/learn/article/charging_lithium_ion_batteries> [↑](#footnote-ref-2)
3. 1C is equal to the charge of the battery divide by 1 hour (Take the Ah of the battery and drop the “h”) [↑](#footnote-ref-3)
4. Requirement EPS-021 [↑](#footnote-ref-4)
5. Requirement REQ-009 [↑](#footnote-ref-5)
6. Requirement EPS-008 [↑](#footnote-ref-6)
7. Requirements EPS-005, EPS-006, EPS-009 [↑](#footnote-ref-7)
8. Requirements EPS-020 [↑](#footnote-ref-8)
9. Requirement EPS-001 [↑](#footnote-ref-9)
10. Requirement EPS-008 [↑](#footnote-ref-10)
11. Requirements EPS-008, EPS-011, EPS-012 [↑](#footnote-ref-11)
12. Requirements EPS-013 [↑](#footnote-ref-12)
13. Requirement EPS-022 [↑](#footnote-ref-13)
14. Requirement EPS-018 [↑](#footnote-ref-14)
15. Requirement EPS-019 [↑](#footnote-ref-15)
16. Requirement EPS-014 [↑](#footnote-ref-16)
17. Requirements EPS-011, EPS-015, EPS-016, EPS-017 [↑](#footnote-ref-17)
18. CIS PN: [60-0014](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/60%20-%20Power%20IC/60-0014) [↑](#footnote-ref-18)
19. CIS PN: [60-0015](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/60%20-%20Power%20IC/60-0015) [↑](#footnote-ref-19)
20. CIS PN: [60-0015](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/60%20-%20Power%20IC/60-0015) [↑](#footnote-ref-20)
21. CIS PN: [01-0001](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/01%20-%20Battery/01-0001) [↑](#footnote-ref-21)
22. CIS PN: [60-0006](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/60%20-%20Power%20IC/60-0006) [↑](#footnote-ref-22)
23. CIS PN: [56-0005](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/56%20-%20Transistor%20FET/56-0005) [↑](#footnote-ref-23)
24. CIS PN: [08-0002](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/08%20-%20Amplifier%20(excluding%20RF)/08-0002) [↑](#footnote-ref-24)
25. CIS PN: [06-0004](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/60%20-%20Power%20IC/60-0004) [↑](#footnote-ref-25)
26. CIS PN: [60-0014](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/60%20-%20Power%20IC/60-0014) [↑](#footnote-ref-26)
27. CIS PN: [08-0003](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/08%20-%20Amplifier%20(excluding%20RF)/08-0003) and [08-0004](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/08%20-%20Amplifier%20(excluding%20RF)/08-0004) [↑](#footnote-ref-27)
28. CIS PN: [60-0014](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/60%20-%20Power%20IC/60-0014) [↑](#footnote-ref-28)
29. CIS PN: [61-0002](https://github.com/CougsInSpace/Resources/tree/cad-libraries/SupplierDocuments/61%20-%20%C2%B5Controller%20(and%20CLPD%2C%20FPGA%2C%20%20etc.)/61-0002) [↑](#footnote-ref-29)
30. For more details on SWD, <https://developer.arm.com/products/system-ip/coresight-debug-and-trace/coresight-architecture/serial-wire-debug> [↑](#footnote-ref-30)
31. For more details on JTAG, <https://en.wikipedia.org/wiki/JTAG> [↑](#footnote-ref-31)
32. CIS PN: [09-0001](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/09%20-%20Communication%20IC/09-0001) [↑](#footnote-ref-32)
33. CIS PN: [09-0001](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/09%20-%20Communication%20IC/09-0001) [↑](#footnote-ref-33)
34. CIS PN: [27-0003](https://github.com/CougsInSpace/Resources/tree/cad-libraries/SupplierDocuments/27%20-%20Conversion%20IC/27-0003) [↑](#footnote-ref-34)
35. CIS PN: [27-0004](https://github.com/CougsInSpace/Resources/tree/cad-libraries/SupplierDocuments/27%20-%20Conversion%20IC/27-0004) [↑](#footnote-ref-35)
36. CIS PN: [08-0002](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/08%20-%20Amplifier%20(excluding%20RF)/08-0002) [↑](#footnote-ref-36)
37. See backplane documentation for details [↑](#footnote-ref-37)
38. For test 3.1, place files in the subfolder *“3.1”* and so on [↑](#footnote-ref-38)
39. Power Line Cycles: DMM setting to average during 100 cycles of the 60Hz wall outlet [↑](#footnote-ref-39)
40. Multilayer Ceramic Capacitor, CIS PN 13-106A [↑](#footnote-ref-40)
41. Power Line Cycles: DMM setting to average during 100 cycles of the 60Hz wall outlet [↑](#footnote-ref-41)