Joshua Lungstrom

This document explains the function of the -Z Panel, its schematic level design, its board level design, and its functional testing

-Z Panel

Revision: 1.0.6



Table of Contents

[1 Introduction 1](#_Toc33355596)

[1.1 Functions 1](#_Toc33355597)

[1.2 Requirements 1](#_Toc33355598)

[2 Detailed Description 2](#_Toc33355599)

[2.1 Functional Block Diagram 2](#_Toc33355600)

[2.1.1 Photodiode 2](#_Toc33355601)

[2.1.2 Analog-to-Digital Converter 3](#_Toc33355602)

[2.2 Schematic 3](#_Toc33355603)

[2.2.1 Isolated Grounds 3](#_Toc33355604)

[2.2.2 Photodiode 3](#_Toc33355605)

[2.2.3 Analog-to-Digital Converter 3](#_Toc33355606)

[2.3 Board 3](#_Toc33355607)

[2.3.1 Layout Constraints 3](#_Toc33355608)

[3 Testing 5](#_Toc33355609)

[3.1 Photodiode 5](#_Toc33355610)

[3.1.1 Test Instructions 5](#_Toc33355611)

[3.1.2 Test Data 5](#_Toc33355612)

[3.1.3 Test Notes 5](#_Toc33355613)

# Introduction

This document explains how the -Z Panel will fulfill the following Functions and conform to the following Requirements. This document refers to the -Z Panel version 1.0.

## Functions

The -Z Panel is responsible for the following:

* Provide the high gain communication antenna
* Provide a Sun sensor for the [ADCS](https://github.com/CougsInSpace/CougSat1-Hardware/blob/master/CougSat1-AvionicBoard/Documentation/ADCS-Design.pdf)

## Requirements

The system requirements and -Z panel requirements can be found [here](https://github.com/CougsInSpace/CougSat1-Readme/blob/master/CougSat1-Requirements.pdf).

# Detailed Description

This section references the -Z panel [schematic](https://github.com/CougsInSpace/CougSat1-Hardware/blob/master/CougSat1-RadioBoard/Documentation/-ZPanel.pdf). Page numbers will be listed and may have coordinates listed (number and letter combination found around the frame).

## Functional Block Diagram

The block diagram can be found on the first page of the schematic.

### Photodiode

The photodiode is used as a sun sensor for the ADCS to determine the location of the sun.

### Analog-to-Digital Converter

The analog to digital converter (ADC) converts the photodiode analog signal to a digital signal for the ADCS .

## Schematic

### Isolated Grounds

Power ground (PGND) is connected to the EPS circuits for the Antenna Deploy Release. Digital ground (DGND) connects to the ADCS connector as the reference for its I2C bus. Analog ground (AGND) connects to analog monitoring circuits including the ADCs, their voltage reference, and the thermistors. Analog ground is connected to digital ground using a resistor rated up to , the expected current is less than . Chassis ground (CHASSIS) is connected to the mechanical features including bolt holes.

### Photodiode

The photodiode[[1]](#footnote-1) can be found on page 2 (A1) of the schematic connected to the ADC. This photodiode is connected through the ADC to the ADCS system. This photodiode has a spectral sensitivity of and the expected illuminance is on the order of < . This makes the expected voltage drop across the load resistor about .

### Analog-to-Digital Converter

The ADC[[2]](#footnote-2) is located on page 2 (A2) of the schematic. The ADC connects the photodiode to the ADCS for determining the location of the sun. The remaining ADC inputs are used to measure temperature at various locations on the board.

## Board

The board shall be double layered with copper, ENIG finish, and thick.

### Layout Constraints

Unless specified in the following subsections, all signals shall use the default parameters specified below. Signals in the following subsections do not include their sense signals unless specified. Trace width can be broken if a trace needs to bottleneck down to a pin, the bottleneck shall be minimized.

Trace width: 0.2𝑚𝑚

Vias: 0.3𝑚𝑚, unlimited count

Separation: 0.2𝑚𝑚

Length: unlimited

#### I2C-I2C\_[SDA, SCL]

Length: Each node shall be length matched ±1.0𝑚𝑚

Stubs: < 10.0𝑚𝑚

# Testing

All tests shall be performed at room temperature and not under vacuum unless otherwise specified. If any modifications are performed, take note. Include enough information to understand circuit behavior and for others to replicate the results. Include any software written to execute the test and link it in the test notes section. Save all software, waveforms, etc. in a subfolder of the board’s test folder for each test.

* Waveforms shall be captured whenever appropriate
* Have the event take fill the screen (for fast events, zoom in; for slow events, zoom out)
* Label each channel accurately
* Only have bandwidth limiting if necessary for the test (this applies to the oscilloscope and probe settings)
* If ringing or overshoot occurs, use a ground spring or differential probe

Results location: <https://github.com/CougsInSpace/CougSat1-Hardware/tree/master/CougSat1-RadioBoard/Testing/+XPanel.1.0>

Common test instructions can be found on the [wiki](http://cougs.space/wiki).

## Photodiode

**Results: Pass/Fail**

**Configuration:**

This test evaluates the circuit described in Photodiode.

### Test Instructions

Connect the ADC to the ADCS. Illuminate the photodiode with a bright light, measure the output voltage. Repeat with a dim light and a dark room. Verify the voltage changes accordingly

### Test Data

| Test the photodiode’s response | | | |
| --- | --- | --- | --- |
| Light source | Voltage | Passing Criteria | Pass / Fail |
| Dark room Or shaded |  |  |  |
| Dim light |  |  |  |
| Bright light |  |  |  |

### Test Notes

Delete me if no notes are required.

1. CIS PN: [66-0003](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/66%20-%20Sensor/66-0003) [↑](#footnote-ref-1)
2. CIS PN: [27-0003](https://github.com/CougsInSpace/Resources/tree/master/SupplierDocuments/27%20-%20Conversion%20IC/27-0003) [↑](#footnote-ref-2)